Zen API | Contents | Reference |

zIndicatorSet constants Macros
zIndicatorSet constants
Macros

Macro | Description
zEVENT_1X_APP_VERSION | Firmware application version (master).
zEVENT_1X_ENCODER_INDEX | Current encoder index count.
zEVENT_1X_ENCODER_VALUE | Current encoder tick count.
zEVENT_1X_INPUT_STATES | Current digital input states.
zEVENT_ENCODER_INDEX | Current encoder index count.
zEVENT_ENCODER_VALUE | Current encoder tick count.
zEVENT_INPUT_STATES | Current digital input states.
zHEALTH_1X_SENSOR_APP_VERSION | Firmware application version.
zHEALTH_1X_SENSOR_CAMERA_ERRORS | Camera error count.
zHEALTH_1X_SENSOR_CAMERA_LOSSES | Camera frame loss count.
zHEALTH_1X_SENSOR_CAMERA_STATUS | Camera status (0: Normal, 1: Error).
zHEALTH_1X_SENSOR_DATA_ERRORS | Data error count.
zHEALTH_1X_SENSOR_DATA_LOSSES | Data loss count.
zHEALTH_1X_SENSOR_DATA_STATUS | Data communication status (sensor-to-station; 0: Normal, 1: Error).
zHEALTH_1X_SENSOR_MEMORY_USAGE | Amount of memory currently used (percentage).
zHEALTH_1X_SENSOR_SYNC_ERRORS | Synchronization error count.
zHEALTH_1X_SENSOR_SYNC_STATUS | Synchronization status (master-to-sensor; 0: Normal, 1: Error).
zHEALTH_1X_SENSOR_TEMPERATURE | Internal temperature (degrees Celsius).
zHEALTH_1X_SENSOR_VOLTAGE_ERRORS | Sensor voltage error count.
zHEALTH_1X_SENSOR_VOLTAGE_STATUS | Sensor voltage status (0: Normal, 1: Error).
zHEALTH_1X_SERVER_APP_VERSION | Firmware application version.
zHEALTH_1X_SERVER_COMM_STATUS | Server communication status (0: Normal, 1: Error).
zHEALTH_1X_SERVER_DATA_LOSSES | Server data loss count.
zHEALTH_1X_SERVER_ENCODER_FREQUENCY | Current encoder frequency (ticks/s).
zHEALTH_1X_SERVER_ENCODER_INDEX | Current encoder index count.
zHEALTH_1X_SERVER_ENCODER_VALUE | Current encoder tick count.
zHEALTH_1X_SERVER_INPUT_STATES | Current digital input states.
zHEALTH_1X_SERVER_NET_OUT_USAGE | Current outbound network throughput (bytes/s).
zHEALTH_1X_SERVER_RESTARTS | Count of system restarts due to errors.
zHEALTH_1X_SERVER_SENSOR_COMM_STATUS | Sensor communication status (0: Normal, 1: Error).
zHEALTH_1X_SERVER_SENSOR_DATA_LOSSES | Sensor data loss count.
zHEALTH_1X_SERVER_SENSOR_RESTARTS | Count of sensor restarts due to errors.
zHEALTH_1X_SERVER_SENSOR_STATE | Current sensor state (1: Error, 2: Ready, 3: Running, 4: Paused, 5: Boot failure).
zHEALTH_1X_SERVER_START_DELAY | Response time for most recent start command (us).
zHEALTH_1X_SERVER_STATE | Current server state (1: Error, 2: Ready, 3: Running, 4: Paused, 5: Boot failure).
zHEALTH_1X_SERVER_TEMPERATURE | Internal temperature (degrees Celsius).
zHEALTH_1X_SERVER_UPTIME | Time elapsed since server boot-up or reset (microseconds).
zHEALTH_MASTER_APP_VERSION | Firmware application version.
zHEALTH_MASTER_FIRESYNC_VERSION | FireSync platform version.
zHEALTH_MASTER_TEMPERATURE | Internal temperature (degrees Celsius).
zHEALTH_SENSOR_APP_VERSION | Firmware application version.
zHEALTH_SENSOR_CAMERA_DROPS | Number of camera frames dropped (does not include errors).
zHEALTH_SENSOR_CAMERA_ERRORS | Number of camera frame errors encountered.
zHEALTH_SENSOR_CAMERA_SPEED | Camera sampling rate, in Hz.
zHEALTH_SENSOR_COMPONENT_VERSION | FireSync platform version.
zHEALTH_SENSOR_CPU_USAGE | CPU usage (percentage of maximum).
zHEALTH_SENSOR_MEMORY_CAPACITY | Total amount of memory available (bytes).
zHEALTH_SENSOR_MEMORY_USAGE | Amount of memory currently used (bytes).
zHEALTH_SENSOR_MESSAGE_IN_DROPS | Number of messages received from acquisition sources, but dropped before data processing.
zHEALTH_SENSOR_MESSAGE_OUT_DROPS | Number of messages generated but not sent.
zHEALTH_SENSOR_NET_OUT_CAPACITY | Total available outbound network throughput (bytes/s).
zHEALTH_SENSOR_NET_OUT_USAGE | Current outbound network throughput (bytes/s).
zHEALTH_SENSOR_STATE | Current node state (1: Error, 2: Ready, 3: Running, 4: Paused).
zHEALTH_SENSOR_STORAGE_CAPACITY | Total amount of non-volatile storage available (bytes).
zHEALTH_SENSOR_STORAGE_USAGE | Amount of non-volatile storage used (bytes).
zHEALTH_SENSOR_SYNC_ERRORS | Number of synchronization errors.
zHEALTH_SENSOR_SYNC_SOURCE | Synchronization source (1: None, 2: Master, 3: Sensor).
zHEALTH_SENSOR_TEMPERATURE | Internal temperature (degrees Celsius).
zHEALTH_SENSOR_TRIGGER_DROPS | Number of input triggers dropped.
zHEALTH_SENSOR_UPTIME | Time elapsed since node boot-up or reset (microseconds).
zHEALTH_SERVER_ENCODER_FREQUENCY | Current encoder frequency (ticks/s).
zHEALTH_SERVER_ENCODER_INDEX | Current encoder index count.
zHEALTH_SERVER_ENCODER_VALUE | Current encoder tick count.
zHEALTH_SERVER_NODE_COMM_ERRORS | Communication error count for each node.
zHEALTH_SERVER_NODE_COMM_STATUS | Communication status for each node (1: Ok, 2: Missing, 3: Error).
zHEALTH_SERVER_SYSTEM_STATE | System state.
zHEALTH_STATION_APP_VERSION | Firmware application version.
zHEALTH_STATION_CPU_USAGE | CPU usage (percentage of maximum).
zHEALTH_STATION_FIRESYNC_VERSION | FireSync platform version.
zHEALTH_STATION_MEMORY_CAPACITY | Total amount of memory available (bytes).
zHEALTH_STATION_MEMORY_USAGE | Amount of memory currently used (bytes).
zHEALTH_STATION_MESSAGE_IN_DROPS | Number of messages received but dropped before processing.
zHEALTH_STATION_MESSAGE_OUT_DROP | Number of messages generated but not sent.
zHEALTH_STATION_NET_IN_CAPACITY | Total available inbound network throughput (bytes/s).
zHEALTH_STATION_NET_IN_USAGE | Current inbound network throughput (bytes).
zHEALTH_STATION_NET_OUT_CAPACITY | Total available outbound network throughput (bytes/s).
zHEALTH_STATION_NET_OUT_USAGE | Current outbound network throughput (bytes/s).
zHEALTH_STATION_STATE | Current node state (1: Error, 2: Ready, 3: Running, 4: Paused).
zHEALTH_STATION_STORAGE_CAPACITY | Total amount of non-volatile storage available (bytes).
zHEALTH_STATION_STORAGE_USAGE | Amount of non-volatile storage used (bytes).
zHEALTH_STATION_UPTIME | Time elapsed since node boot-up or reset (microseconds).

Copyright (c) 2008-2010 by LMI Technologies Inc. All rights reserved.
Contents | Reference