Gocator API > Go2 > Values

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Values
Enumerations Go2 Structures Types

Go2 Values

Enumerations

Enumeration | Description
Go2Axis | Represents a coordinate axis (X, Y, or Z).
Go2CalibrationState | Represents the calibration status of a sensor system.
Go2CalibrationTarget | Represents a calibration target type.
Go2Changes | Represents changes in the sensor system that require a client refresh.
Go2ConnectionType | Represents the type of system interconnection.
Go2DataSource | Represents a data source source.
Go2EncoderPeriodMinSource | Determines what is currently limiting the minimum encoder period.
Go2EncoderTriggerMode | Represents an encoders triggering behavior.
Go2ExposureMode | Represents an Exposure Mode type.
Go2FrameRateMaxSource | Determines what is currently limiting the maximum frame rate.
Go2Mode | Represents an operation mode.
Go2Orientation | Represents a sensor orientation type.
Go2ResamplingType | Represents resampling behavior
Go2SensorOrientation | Represents the sensors orientation
Go2SensorPairState | Represents the pair state of a sensor
Go2SensorRole | Represents the current role of a sensor within a sensor system.
Go2Side | Abstract representation of sides
Go2SystemDomain | Represents the systems primary synchronization domain
Go2SystemState | Represents the state of the sensor system.
Go2TriggerSource | Represents a trigger source type.
Go2User | Represents a user id.

Structures

Structure | Description
Go2AddressInfo | Network address settings for a sensor.

Types

Type | Description
Go2Bool | Boolean value.
Go2Byte | One Byte.
Go2Char | 8-bit ASCII character.
Go2Double | Double-precision floating-point number.
Go2Float | Single-precision floating-point number.
Go2Handle | Handle to an object instance.
Go2Int16 | 16-bit signed integer.
Go2Int32 | 32-bit signed integer.
Go2Int64 | 64-bit signed integer.
Go2Int8 | 8-bit signed integer.
Go2IntPtr | Signed integer that can store a pointer address difference.
Go2IPAddress | Represents an IPv4 Address.
Go2Status | Represents an error code.
Go2Type | Represents a type identifier.
Go2UInt16 | 16-bit unsigned integer.
Go2UInt32 | 32-bit unsigned integer.
Go2UInt64 | 64-bit unsigned integer.
Go2UInt8 | 8-bit unsigned integer.
Go2UIntPtr | Unsigned integer that can store a pointer address.
Go2Version | Represents a version number.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference