Gocator API > Go2.Output > Values > Go2DigitalSignalType

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2DigitalSignalType
Values
Description

Type of output. Only applies when output is based on measurements.

C

    enum Go2DigitalSignalType {
      GO2_DIGITAL_SIGNAL_TYPE_PULSED = 0,
      GO2_DIGITAL_SIGNAL_TYPE_CONTINUOUS = 1
    };

Members

Members | Description
GO2_DIGITAL_SIGNAL_TYPE_PULSED = 0 | Digital output is pulsed.
GO2_DIGITAL_SIGNAL_TYPE_CONTINUOUS = 1 | Digital output is latched continuously until driven low.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference