Gocator API > Go2.Output > Values > Go2DigitalPassMode

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2DigitalPassMode
Values
Description

Represents digital output triggering behavior.

C

    enum Go2DigitalPassMode {
      GO2_DIGITAL_PASS_MODE_TRUE = 0,
      GO2_DIGITAL_PASS_MODE_FALSE = 1,
      GO2_DIGITAL_PASS_MODE_ALWAYS = 2
    };

Members

Members | Description
GO2_DIGITAL_PASS_MODE_TRUE = 0 | Digital output is asserted on decision pass.
GO2_DIGITAL_PASS_MODE_FALSE = 1 | Digital output is asserted on decision fail.
GO2_DIGITAL_PASS_MODE_ALWAYS = 2 | Digital output is asserted on decision pass or fail.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference