Gocator API > Go2.Output > Classes > Go2Serial > Functions

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2Serial

Go2Serial functions.

Functions

Function | Description
Go2Serial_AddSource | Selects the specified source for transmission.
Go2Serial_AsciiCustomDataFormat | Gets the ASCII custom format.
Go2Serial_AsciiCustomFormatEnabled | Reports whether the ASCII custom data format is currently enabled. This setting only applies when the operation is asynchronous. When enabled, the measurements selected via add/remove source are ignored.
Go2Serial_AsciiDelimiter | Gets the string used to delimit tokens in standard formatted data.
Go2Serial_AsciiInvalid | Gets the string used represent invalid values.
Go2Serial_AsciiTerminator | Gets the string used to terminate commands and standard formatted data.
Go2Serial_ClearSources | Removes all selected sources for the specified output type.
Go2Serial_EnableAsciiCustomFormat | Enables the ASCII custom data format to allow user-specified formatting of the data string.
Go2Serial_OptionAt | Gets the source option at the specified index.
Go2Serial_OptionCount | Gets the number of source options for the specified output type.
Go2Serial_Protocol | Gets the protocol that the serial follows.
Go2Serial_RemoveSource | Removes (deselects) the source at the specified index.
Go2Serial_SelcomDataScaleMax | Gets the measurement value associated with the maximum Selcom value.
Go2Serial_SelcomDataScaleMin | Gets the measurement value associated with the minimum Selcom value.
Go2Serial_SelcomFormat | Gets the format that Selcom serial uses.
Go2Serial_SelcomFormatOptionAt | Gets a specified selcom format option.
Go2Serial_SelcomFormatOptionCount | Gets the total number of selcom format options.
Go2Serial_SelcomRate | Gets the Selcom signaling rate.
Go2Serial_SelcomRateOptionAt | Gets a specified rate option.
Go2Serial_SelcomRateOptionCount | Gets the total number of rate options.
Go2Serial_SetAsciiCustomDataFormat | Sets the custom ASCII format.
Go2Serial_SetAsciiDelimiter | Sets the string used to delimit tokens in standard formatted data.
Go2Serial_SetAsciiInvalid | Sets the string used represent invalid values.
Go2Serial_SetAsciiTerminator | Sets the string used to terminate commands and standard formatted data.
Go2Serial_SetProtocol | Sets the protocol that the serial follows.
Go2Serial_SetSelcomDataScaleMax | Sets the measurement value associated with the maximum Selcom value.
Go2Serial_SetSelcomDataScaleMin | Sets the measurement value associated with the minimum Selcom value.
Go2Serial_SetSelcomFormat | Sets the format that Selcom serial uses.
Go2Serial_SetSelcomRate | Sets the Selcom signaling rate.
Go2Serial_SourceAt | Gets the identifier of the selected output source at the specified index.
Go2Serial_SourceCount | Gets the number of sources of the specified output type that are currently selected for transmission.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference