Gocator API > Go2.Output > Classes > Go2Serial > Functions > Go2Serial_SetSelcomRate

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2Serial_SetSelcomRate
Functions
Description

Sets the Selcom signaling rate.

C

    Go2Status Go2Serial_SetSelcomRate(Go2Serial serial, Go2UInt32 rate);

Parameters

Parameters | Description
Go2Serial serial | Go2Serial object.
Go2UInt32 rate | The Selcom signaling rate.

Returns

Operation status.

File

Go2OutputChannels.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference