Zen API | Contents | Reference | Previous | Up | Next

zFireSync_StartActiveHealth
zFireSync functions
C

    zStatus zFireSync_StartActiveHealth(zFireSync fireSync, zIPAddress receiver, z32u port);

Parameters

Parameters | Description
zFireSync fireSync | zFireSync object.
zIPAddress receiver | IP address of health receiver.
z32u port | Port at which the health receiver is listening.

Description

Commands FireSync server to begin sending health messages to specified receiver.

Remarks

This function uses the Management channel.

If this call is successful, FireSync server will open a connection to the specified port and begin transmitting health messages. A zReceiver object can be used to accept the incoming connection from FireSync server and to receive health messages.

File

zFireSync.h

Copyright (c) 2008-2010 by LMI Technologies Inc. All rights reserved.
Contents | Reference