Gocator API > Go2 > Values > Go2Changes

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2Changes
Values
Description

Represents changes in the sensor system that require a client refresh.

C

    enum Go2Changes {
      GO2_CHANGES_NONE = 0x00,
      GO2_CHANGES_DEVICE = 0x02,
      GO2_CHANGES_CONNECTION = 0x04
    };

Members

Members | Description
GO2_CHANGES_NONE = 0x00 | No changes - client state is consistent with system state.
GO2_CHANGES_DEVICE = 0x02 | One or more devices have come online or gone offline - refresh required.
GO2_CHANGES_CONNECTION = 0x04 | Client has been disconnected - refresh required.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference