Zen API | Contents | Reference | Previous | Up | Next

zFireSync_StartActiveEvents
zFireSync functions
C

    zStatus zFireSync_StartActiveEvents(zFireSync fireSync, zIPAddress receiver, z32u port);

Parameters

Parameters | Description
zFireSync fireSync | zFireSync object.
zIPAddress receiver | IP address of event receiver.
z32u port | Port at which the event receiver is listening.

Description

Commands FireSync server to begin sending event messages to specified receiver.

Remarks

This function uses the Control channel.

If this call is successful, FireSync server will open a connection to the specified port and begin transmitting event messages. A zReceiver object can be used to accept the incoming connection from FireSync server and to receive event messages.

File

zFireSync.h

Copyright (c) 2008-2010 by LMI Technologies Inc. All rights reserved.
Contents | Reference