Gocator API > Go2.Output > Values

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Values
Enumerations Go2.Output

Go2.Output Values

Enumerations

Enumeration | Description
Go2AnalogEvent | Represents the event which triggers this output.
Go2AnalogTriggerMode | Represents Analog output triggering behavior.
Go2AsciiOperation | Represents the operation used by ASCII protocol
Go2DigitalEvent | Represents the event which triggers this output.
Go2DigitalPassMode | Represents digital output triggering behavior.
Go2DigitalSignalType | Type of output. Only applies when output is based on measurements.
Go2EthernetProtocol | Represents the protocol followed on the ethernet
Go2OutputDataSourceType | Represents the type of output data source.
Go2SelcomFormat | Represents the selcom format followed on the serial output
Go2SerialProtocol | Represents the protocol followed on the serial output

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference