Gocator API > Go2.Part > Classes > Go2Part > Functions

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2Part

Go2Part Functions

Functions

Function | Description
Go2Part_AddMeasurement | Creates a new part measurement and adds it to the list of measurements.
Go2Part_AreaThreshold | Gets the minimum area threshold for part detection.
Go2Part_AreaThresholdLimitMax | Gets the maximum valid value for the AreaMin setting.
Go2Part_AreaThresholdLimitMin | Gets the minimum valid value for the AreaMin setting.
Go2Part_ClearMeasurements | Removes all part measurements.
Go2Part_FrameOfReference | Gets the frame of reference type.
Go2Part_GapThreshold | Gets the Gap Threshold for part detection.
Go2Part_GapThresholdLimitMax | Gets the maximum valid value for the Gap Threshold setting.
Go2Part_GapThresholdLimitMin | Gets the minimum valid value for the Gap Threshold setting.
Go2Part_HeightThreshold | Gets the minimum height threshold for part detection.
Go2Part_HeightThresholdDirection | Gets the direction of the height threshold.
Go2Part_HeightThresholdLimitMax | Gets the maximum valid value for the HeightThreshold setting.
Go2Part_HeightThresholdLimitMin | Gets the minimum valid value for the HeightThreshold setting.
Go2Part_LengthMax | Gets the maximum length for part detection.
Go2Part_LengthMaxLimitMax | Gets the maximum valid value for the LengthMax setting.
Go2Part_LengthMaxLimitMin | Gets the minimum valid value for the LengthMax setting.
Go2Part_MeasurementAt | Gets the part measurement at the specified index;
Go2Part_MeasurementCount | Gets the current count of part measurements.
Go2Part_RemoveMeasurement | Removes the part measurement at the specified index.
Go2Part_SetAreaThreshold | Sets the minimum area threshold for part detection.
Go2Part_SetFrameOfReference | Set the frame of reference for detected parts.
Go2Part_SetGapThreshold | Sets the Gap Threshold for part detection.
Go2Part_SetHeightThreshold | Set the minimum height threshold for part detection.
Go2Part_SetHeightThresholdDirection | Set the height threshold direction for part detection.
Go2Part_SetLengthMax | Sets the maximum length for part detection.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference