Gocator API > Go2.Output > Classes > Go2Digital > Functions > Go2Digital_SetDelay

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2Digital_SetDelay
Functions
Description

Sets the delay from exposure until output is triggered, in units based on SyncDomain. mm when SyncDomain is distance, us when SyncDomain is time. Ignored when SyncDomain is Immediate or when PassMode is Software

C

    Go2Status Go2Digital_SetDelay(Go2Digital digital, Go2Int64 delay);

Parameters

Parameters | Description
Go2Digital digital | Go2Digital object.
Go2Int64 delay | The delay (us or mm)

Returns

Operation status.

File

Go2OutputChannels.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference