Gocator API > Go2.Output > Classes > Go2Ethernet > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2Ethernet_AddSource | Selects the specified source for transmission.
Go2Ethernet_AsciiControlPort | Gets the port used for control.
Go2Ethernet_AsciiCustomDataFormat | Gets the ASCII custom format.
Go2Ethernet_AsciiCustomFormatEnabled | Reports whether the ASCII custom data format is currently enabled. This setting only applies when the operation is asynchronous. When enabled, the measurements selected via add/remove source are ignored.
Go2Ethernet_AsciiDataPort | Gets the port used for data.
Go2Ethernet_AsciiDelimiter | Gets the string used to delimit tokens in commands and standard formatted data.
Go2Ethernet_AsciiHealthPort | Gets the port used for health.
Go2Ethernet_AsciiInvalid | Gets the string used represent invalid values.
Go2Ethernet_AsciiOperation | Gets the ASCII operation.
Go2Ethernet_AsciiTerminator | Gets the string used to terminate commands and standard formatted data.
Go2Ethernet_ClearSources | Removes all selected sources for the specified output type.
Go2Ethernet_EIPBufferEnabled | Reports whether the EthernetIP output buffer is currently enabled.
Go2Ethernet_EnableAsciiCustomFormat | Enables or disables the ASCII custom data format to allow user-specified formatting of the data string.
Go2Ethernet_EnableEIPBuffer | Enables or disables the EthernetIP output buffer.
Go2Ethernet_EnableModbusBuffer | Enables or disables the Modbus output buffer.
Go2Ethernet_ModbusBufferEnabled | Reports whether the Modbus output buffer is currently enabled.
Go2Ethernet_OptionAt | Gets the source option at the specified index.
Go2Ethernet_OptionCount | Gets the number of source options for the specified output type.
Go2Ethernet_Protocol | Gets the protocol that the ethernet follows.
Go2Ethernet_RemoveSource | Removes (deselects) the source at the specified index.
Go2Ethernet_SetAsciiControlPort | Sets the port used for control.
Go2Ethernet_SetAsciiCustomDataFormat | Sets the custom ASCII format.
Go2Ethernet_SetAsciiDataPort | Sets the port used for data.
Go2Ethernet_SetAsciiDelimiter | Sets the string used to delimit tokens in commands and standard formatted data.
Go2Ethernet_SetAsciiHealthPort | Sets the port used for health.
Go2Ethernet_SetAsciiInvalid | Sets the string used represent invalid values.
Go2Ethernet_SetAsciiOperation | Sets the ASCII operation. When set to GO2_ASCII_ASYNCHRONOUS, the data port will send data asynchronously according to AsciiCustomFormatEnabled. When set to GO2_ASCII_POLLING, no data will be sent unless requested.
Go2Ethernet_SetAsciiTerminator | Sets the string used to terminate commands and standard formatted data.
Go2Ethernet_SetProtocol | Sets the protocol that the ethernet follows.
Go2Ethernet_SourceAt | Gets the identifier of the selected output at the specified index.
Go2Ethernet_SourceCount | Gets the number of sources of the specified output type that are currently selected for transmission.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference