Gocator API > Go2 > Classes > Go2System > Functions > Go2System_ReceiveData

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2System_ReceiveData
Functions
Description

Waits to receive a data message from the sensor's data channel.

C

    Go2Status Go2System_ReceiveData(Go2System system, Go2UInt64 timeout, Go2Data* data);

Parameters

Parameters | Description
Go2System system | Go2System object.
Go2UInt64 timeout | Timeout interval (microseconds).
Go2Data* data | Receives data message.

Returns

Operation status.

Remarks

Use the Go2System_ConnectData function to start data transmissions. Do not call Go2System_ReceiveData if a callback was provided to the Go2System_ConnectData function.

File

Go2System.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference