Gocator API > Go2 > Values > Go2CalibrationState

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2CalibrationState
Values
Description

Represents the calibration status of a sensor system.

C

    enum Go2CalibrationState {
      GO2_CALIBRATION_STATE_NONE = 0,
      GO2_CALIBRATION_STATE_AUTO = 1,
      GO2_CALIBRATION_STATE_MANUAL = 2
    };

Members

Members | Description
GO2_CALIBRATION_STATE_NONE = 0 | Not calibrated
GO2_CALIBRATION_STATE_AUTO = 1 | Auto calibration has been completed
GO2_CALIBRATION_STATE_MANUAL = 2 | The transformation file has been manually adjusted

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference