Gocator API > Go2.Part > Classes > Go2PartStudTipY > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2PartStudTipY_AutoRefRegionEnabled | Reports whether auto reference regions are enabled.
Go2PartStudTipY_AutoTiltCorrectionEnabled | Reports whether auto tilt correction is enabled.
Go2PartStudTipY_BaseHeight | Gets the height of the base of the stud.
Go2PartStudTipY_DecisionMax | Gets the decision threshold maximum value.
Go2PartStudTipY_DecisionMin | Gets the decision threshold minimum value.
Go2PartStudTipY_EnableAutoRefRegion | Enables or disables auto reference regions.
Go2PartStudTipY_EnableAutoTiltCorrection | Enables or disables auto tilt correction.
Go2PartStudTipY_EnableHold | Enables measurement value hold.
Go2PartStudTipY_EnableLink | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement.
Go2PartStudTipY_EnableRefRegions | Enables or disables the optional reference region.
Go2PartStudTipY_EnableRegion | Enables or disables the optional region.
Go2PartStudTipY_EnableSmoothing | Enables measurement value smoothing.
Go2PartStudTipY_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartStudTipY_Id | Gets the unique measurement identifier for the measurement.
Go2PartStudTipY_Link | Gets the measurement id of the linked measurement.
Go2PartStudTipY_LinkEnabled | Reports whether measurement linking is enabled.
Go2PartStudTipY_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2PartStudTipY_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2PartStudTipY_Name | Gets the descriptive name for the measurement.
Go2PartStudTipY_Offset | Gets the measurement value offset.
Go2PartStudTipY_RefRegionAt | Gets the reference region object at the specified index.
Go2PartStudTipY_RefRegionCount | Gets the number of reference regions.
Go2PartStudTipY_RefRegionsEnabled | Returns the current state of the optional reference region.
Go2PartStudTipY_Region | Gets the region object which defines the measurement's ROI.
Go2PartStudTipY_RegionEnabled | Returns the current state of the optional region.
Go2PartStudTipY_Scale | Gets the measurement value scale factor.
Go2PartStudTipY_SetBaseHeight | Sets the height of the base of the stud.
Go2PartStudTipY_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartStudTipY_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartStudTipY_SetId | Sets the unique measurement identifier for the measurement.
Go2PartStudTipY_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartStud_? measurements)
Go2PartStudTipY_SetName | Sets the descriptive name for the measurement.
Go2PartStudTipY_SetOffset | Sets the measurement value offset.
Go2PartStudTipY_SetRefRegionCount | Sets the number of reference regions to use.
Go2PartStudTipY_SetScale | Sets the measurement value scale factor.
Go2PartStudTipY_SetSmoothingWindow | Sets the smoothing window value.
Go2PartStudTipY_SetStudHeight | Sets the height of the stud to measure.
Go2PartStudTipY_SetStudRadius | Sets the radius of the stud to measure.
Go2PartStudTipY_SetTiltXAngle | Sets the X axis tilt angle.
Go2PartStudTipY_SetTiltYAngle | Sets the Y axis tilt angle.
Go2PartStudTipY_SetTipHeight | Sets the height of the tip of the stud.
Go2PartStudTipY_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartStudTipY_SmoothingWindow | Gets the smoothing window value.
Go2PartStudTipY_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartStudTipY_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2PartStudTipY_StudHeight | Gets the height of the stud to measure.
Go2PartStudTipY_StudRadius | Gets the radius of the stud to measure.
Go2PartStudTipY_TiltXAngle | Gets the X axis tilt angle.
Go2PartStudTipY_TiltYAngle | Gets the Y axis tilt angle.
Go2PartStudTipY_TipHeight | Gets the height of the tip of the stud.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference