Gocator API > Go2.Output > Values > Go2AnalogTriggerMode

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2AnalogTriggerMode
Values
Description

Represents Analog output triggering behavior.

C

    enum Go2AnalogTriggerMode {
      GO2_ANALOG_TRIGGER_MODE_MEASUREMENT = 0,
      GO2_ANALOG_TRIGGER_MODE_SOFTWARE = 1
    };

Members

Members | Description
GO2_ANALOG_TRIGGER_MODE_MEASUREMENT = 0 | Analog output is set based on measurment selected.
GO2_ANALOG_TRIGGER_MODE_SOFTWARE = 1 | Analog output is software controlled

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference