Gocator API > Go2 > Values > Go2SystemState

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2SystemState
Values
Description

Represents the state of the sensor system.

C

    enum Go2SystemState {
      GO2_SYSTEM_STATE_CONFLICT = 1,
      GO2_SYSTEM_STATE_READY = 2,
      GO2_SYSTEM_STATE_RUNNING = 3
    };

Members

Members | Description
GO2_SYSTEM_STATE_CONFLICT = 1 | System cannot run because of configuration conflicts.
GO2_SYSTEM_STATE_READY = 2 | System is currently stopped, but is ready to run.
GO2_SYSTEM_STATE_RUNNING = 3 | System is running.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference