Gocator API > Go2 > Values > Go2ExposureMode

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2ExposureMode
Values
Description

Represents an Exposure Mode type.

C

    enum Go2ExposureMode {
      GO2_EXPOSURE_MODE_SINGLE = 0,
      GO2_EXPOSURE_MODE_MULTIPLE = 1,
      GO2_EXPOSURE_MODE_DYNAMIC = 2
    };

Members

Members | Description
GO2_EXPOSURE_MODE_SINGLE = 0 | Single exposure mode.
GO2_EXPOSURE_MODE_MULTIPLE = 1 | Multiple exposure mode.
GO2_EXPOSURE_MODE_DYNAMIC = 2 | Dynamic exposure mode.

File

Go2Sensor.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference