Zen API | Contents | Reference | Previous | Up | Next

zFireSync_EnablePassiveData
zFireSync functions
C

    zStatus zFireSync_EnablePassiveData(zFireSync fireSync, z32u dataChannel, zIPEndPoint* sender);

Parameters

Parameters | Description
zFireSync fireSync | zFireSync object.
z32u dataChannel | FireSync server data channel ID (0-63).
zIPEndPoint* sender | IP end point of the passive sender.

Description

Enables a FireSync server passive data channel and provides the end-point to which a receiver can connect.

Remarks

This function uses the Control channel and can be called only when the system is stopped.

A zReceiver object can be used to connect to the FireSync server at the sender address, and to receive data messages. When the zFireSync_Start function is called, the server will send data messages to any connected passive receivers.

File

zFireSync.h

Copyright (c) 2008-2010 by LMI Technologies Inc. All rights reserved.
Contents | Reference