Gocator API > Go2.Profile > Classes > Go2ProfileStripWidth > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2ProfileStripWidth_Area | Gets the region of interest.
Go2ProfileStripWidth_BaseType | Gets the base type of the strip to search for.
Go2ProfileStripWidth_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileStripWidth_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileStripWidth_EdgeHeightMin | Gets the minimum height for an edge to be considered.
Go2ProfileStripWidth_EdgeSupportWidth | Gets the width of the search window to use when detecting edges.
Go2ProfileStripWidth_EdgeTransitionWidth | Gets the width of the expected edge transition.
Go2ProfileStripWidth_EdgeTransitionWidthMax | Gets the maximum value allowable for the edge transition.
Go2ProfileStripWidth_EnableHold | Enables measurement value hold.
Go2ProfileStripWidth_EnableLeftEdgeType | Enables or disables detection of the specified left edge type.
Go2ProfileStripWidth_EnableLink | Enables or disables measurement linking.
Go2ProfileStripWidth_EnableRightEdgeType | Enables or disables detection of the specified right edge type.
Go2ProfileStripWidth_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileStripWidth_EnableTilt | Enables or disables tilt correction.
Go2ProfileStripWidth_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileStripWidth_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileStripWidth_LeftEdgeTypeEnabled | Determines whether the specified left edge type is enabled for detection.
Go2ProfileStripWidth_Link | Gets the measurement id of the linked measurement.
Go2ProfileStripWidth_LinkEnabled | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement. E.g. A Go2PartOpeningX and Go2PartOpeningY measurement can link, but two Go2PartOpeningX measurements can not be linked.
Go2ProfileStripWidth_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2ProfileStripWidth_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2ProfileStripWidth_Name | Gets the descriptive name for the measurement.
Go2ProfileStripWidth_Offset | Gets the measurement value offset.
Go2ProfileStripWidth_RightEdgeTypeEnabled | Determines whether the specified right edge type is enabled for detection.
Go2ProfileStripWidth_Scale | Gets the measurement value scale factor.
Go2ProfileStripWidth_SelectN | Gets the N-th strip to select when selectType is GO2_PROFILE_STRIP_SELECT_LEFT or GO2_PROFILE_STRIP_SELECT_RIGHT.
Go2ProfileStripWidth_SelectType | Gets the select type.
Go2ProfileStripWidth_SetBaseType | Sets the base type of the strip to search for.
Go2ProfileStripWidth_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileStripWidth_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileStripWidth_SetEdgeHeightMin | Sets the minimum height for an edge to be considered.
Go2ProfileStripWidth_SetEdgeSupportWidth | Sets the width of the search window to use when detecting edges.
Go2ProfileStripWidth_SetEdgeTransitionWidth | Sets the width of the expected edge transition.
Go2ProfileStripWidth_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileStripWidth_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2ProfileStripWidth_SetName | Sets the descriptive name for the measurement.
Go2ProfileStripWidth_SetOffset | Sets the measurement value offset.
Go2ProfileStripWidth_SetScale | Sets the measurement value scale factor.
Go2ProfileStripWidth_SetSelectN | Sets the N-th strip to select when selectType is GO2_PROFILE_STRIP_SELECT_LEFT or GO2_PROFILE_STRIP_SELECT_RIGHT.
Go2ProfileStripWidth_SetSelectType | Sets the select type.
Go2ProfileStripWidth_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileStripWidth_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileStripWidth_SetVoidMax | Sets the maximum width of the void that will be ignored.
Go2ProfileStripWidth_SetWidthMin | Sets the minimum width for a strip to be considered.
Go2ProfileStripWidth_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileStripWidth_SmoothingWindow | Gets the smoothing window value.
Go2ProfileStripWidth_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileStripWidth_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileStripWidth_Source | Gets the source for profile data used in this measurement.
Go2ProfileStripWidth_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileStripWidth_SourceOptionCount | Gets the number of profile source options for the measurement.
Go2ProfileStripWidth_TiltEnabled | Determines whether tilt correction is enabled.
Go2ProfileStripWidth_VoidMax | Gets the maximum width of the void that will be ignored.
Go2ProfileStripWidth_VoidMaxLimitMax | Gets the limit for the VoidMax property.
Go2ProfileStripWidth_WidthMin | Gets the minimum width for a strip to be considered.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference