Gocator API > Go2 > Constants

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Constants
Go2 Macros

Go2 Constants

Macros

Macro | Description
GO2_DEFAULT_DHCP | Default sensor DHCP status (disabled).
GO2_DEFAULT_IP_ADDRESS | Default sensor IP address ("192.168.1.10").
GO2_DEFAULT_IP_GATEWAY | Default sensor IP gateway ("0.0.0.0").
GO2_DEFAULT_IP_MASK | Default sensor IP mask ("255.255.255.0").
GO2_INFINITE | Infinity (can be used for timeouts).
GO2_INVALID_RANGE | Value for ranges when they are considered invalid
GO2_MAX_EXPOSURES | Maximum number of multiple exposure steps
GO2_MAX_REF_REGIONS | Represents the maximum number of reference regions that can be returned in certain part measurements
GO2_NIL | Null Go2Handle value.
GO2_NULL | Null pointer value.
GO2_SENSOR_DEVICE_ID_UNKNOWN | Special device id for use when creating sensors without a know id
GO2_SYSTEM_LIVE_BUNDLE_NAME | Current file bundle name
GO2_SYSTEM_LIVE_CONFIG_NAME | Current configuration file name
GO2_SYSTEM_LIVE_TRANSFORM_NAME | Current transform file name

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference