Gocator API > Go2.Output > Values > Go2OutputDataSourceType

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2OutputDataSourceType
Values
Description

Represents the type of output data source.

C

    enum Go2OutputDataSourceType {
      GO2_OUTPUT_DATA_SOURCE_TYPE_NONE = 0,
      GO2_OUTPUT_DATA_SOURCE_TYPE_PROFILE = 1,
      GO2_OUTPUT_DATA_SOURCE_TYPE_PART = 2,
      GO2_OUTPUT_DATA_SOURCE_TYPE_VIDEO = 3,
      GO2_OUTPUT_DATA_SOURCE_TYPE_VALUE = 4,
      GO2_OUTPUT_DATA_SOURCE_TYPE_DECISION = 5,
      GO2_OUTPUT_DATA_SOURCE_TYPE_RAW_PROFILE = 6,
      GO2_OUTPUT_DATA_SOURCE_TYPE_PROFILE_INTENSITY = 7,
      GO2_OUTPUT_DATA_SOURCE_TYPE_RAW_PROFILE_INTENSITY = 8,
      GO2_OUTPUT_DATA_SOURCE_TYPE_PART_INTENSITY = 9,
      GO2_OUTPUT_DATA_SOURCE_TYPE_RANGE = 10,
      GO2_OUTPUT_DATA_SOURCE_TYPE_RANGE_INTENSITY = 11
    };

Members

Members | Description
GO2_OUTPUT_DATA_SOURCE_TYPE_NONE = 0 | No output source.
GO2_OUTPUT_DATA_SOURCE_TYPE_PROFILE = 1 | Output source is profile data. Supported only on 2x00 series sensors.
GO2_OUTPUT_DATA_SOURCE_TYPE_PART = 2 | Output source is part data. Supported only on 2x00 and 3x00 series sensors.
GO2_OUTPUT_DATA_SOURCE_TYPE_VIDEO = 3 | Output source is video data.
GO2_OUTPUT_DATA_SOURCE_TYPE_VALUE = 4 | Output source is measurement value data.
GO2_OUTPUT_DATA_SOURCE_TYPE_DECISION = 5 | Output source is measurement decision data.
GO2_OUTPUT_DATA_SOURCE_TYPE_RAW_PROFILE = 6 | Output source is raw profile data. Supported only on 2x00 series sensors.
GO2_OUTPUT_DATA_SOURCE_TYPE_PROFILE_INTENSITY = 7 | Output source is profile intensity data. Supported only on 2x00 series sensors.
GO2_OUTPUT_DATA_SOURCE_TYPE_RAW_PROFILE_INTENSITY = 8 | Output source is raw profile intensity data. Supported only on 2x00 series sensors.
GO2_OUTPUT_DATA_SOURCE_TYPE_PART_INTENSITY = 9 | Output source is part intensity data. Supported only on 2x00 series sensors.
GO2_OUTPUT_DATA_SOURCE_TYPE_RANGE = 10 | Output source is range data. Supported only on 1x00 series sensors.
GO2_OUTPUT_DATA_SOURCE_TYPE_RANGE_INTENSITY = 11 | Output source is range intensity data. Supported only on 1x00 series sensors.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference