Gocator API > Go2 > Classes > Go2Sensor > Functions > Go2Sensor_SetActiveAreaHeight

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2Sensor_SetActiveAreaHeight
Functions
Description

Sets the active area height.

C

    Go2Status Go2Sensor_SetActiveAreaHeight(Go2Sensor sensor, Go2Double height);

Parameters

Parameters | Description
Go2Sensor sensor | Go2Sensor object.
Go2Double height | Active area height (mm).

Returns

Operation status.

File

Go2Sensor.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference