Gocator API > Go2 > Values > Go2ReferenceImageState

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2ReferenceImageState
Values
Description

Represents whether a reference image has been set. Supported only on 2000 series sensors.

C

    enum Go2ReferenceImageState {
      GO2_REFERENCE_IMAGE_STATE_NONE = 0,
      GO2_REFERENCE_IMAGE_STATE_SET = 1
    };

Members

Members | Description
GO2_REFERENCE_IMAGE_STATE_NONE = 0 | Not set.
GO2_REFERENCE_IMAGE_STATE_SET = 1 | Set.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference