Gocator API > Go2 > Classes > Go2Sensor > Functions

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2Sensor

Go2Sensor functions.

Functions

Function | Description
Go2Sensor_ActiveAreaHeight | Gets the active area height.
Go2Sensor_ActiveAreaHeightMax | Gets the maximum valid value for the ActiveAreaHeight setting.
Go2Sensor_ActiveAreaHeightMin | Gets the minimum valid value for the ActiveAreaHeight setting.
Go2Sensor_ActiveAreaLength | Gets the active area Length.
Go2Sensor_ActiveAreaLengthMax | Gets the maximum valid value for the ActiveAreaLength setting.
Go2Sensor_ActiveAreaLengthMin | Gets the minimum valid value for the ActiveAreaLength setting.
Go2Sensor_ActiveAreaWidth | Gets the active area width.
Go2Sensor_ActiveAreaWidthMax | Gets the maximum valid value for the ActiveAreaWidth setting.
Go2Sensor_ActiveAreaWidthMin | Gets the minimum valid value for the ActiveAreaWidth setting.
Go2Sensor_ActiveAreaX | Gets the active area x origin.
Go2Sensor_ActiveAreaXMax | Gets the maximum valid value for the ActiveAreaX setting.
Go2Sensor_ActiveAreaXMin | Gets the minimum valid value for the ActiveAreaX setting.
Go2Sensor_ActiveAreaY | Gets the active area Y origin.
Go2Sensor_ActiveAreaYMax | Gets the maximum valid value for the ActiveAreaY setting.
Go2Sensor_ActiveAreaYMin | Gets the minimum valid value for the ActiveAreaY setting.
Go2Sensor_ActiveAreaZ | Gets the active area z origin.
Go2Sensor_ActiveAreaZMax | Gets the maximum valid value for the ActiveAreaZ setting.
Go2Sensor_ActiveAreaZMin | Gets the minimum valid value for the ActiveAreaZ setting.
Go2Sensor_AddExposureStep | Adds an exposure step
Go2Sensor_BackCameraHeight | Gets the camera region-of-interest height.
Go2Sensor_BackCameraWidth | Gets the camera region-of-interest width.
Go2Sensor_BackCameraX | Gets the camera region-of-interest x origin.
Go2Sensor_BackCameraY | Gets the camera region-of-interest y origin.
Go2Sensor_CalibratedHeight | Gets the sensor's active area height in system coordinates (post-calibration).
Go2Sensor_CalibratedLength | Gets the sensor's active area length in system coordinates (post-calibration).
Go2Sensor_CalibratedWidth | Gets the sensor's active area width in system coordinates (post-calibration).
Go2Sensor_CalibratedX | Gets the sensor's active area x-origin in system coordinates (post-calibration).
Go2Sensor_CalibratedY | Gets the sensor's active area y-origin in system coordinates (post-calibration).
Go2Sensor_CalibratedZ | Gets the sensor's active area z-origin in system coordinates (post-calibration).
Go2Sensor_ClearExposureSteps | Removes all exposure steps.
Go2Sensor_CustomElement | Gets the XML document representing the custom configuration block within the Sensor block for the Gocator Base Library.
Go2Sensor_EnableExposureTraining | Enables this sensor to be used as a part of training the exposure. Only one sensor in the system may have this enabled at a time.
Go2Sensor_Exposure | Gets the exposure value.
Go2Sensor_ExposureDelay | Gets the exposure delay.
Go2Sensor_ExposureMax | Gets the maximum valid value for the Exposure setting.
Go2Sensor_ExposureMin | Gets the minimum valid value for the Exposure setting.
Go2Sensor_ExposureMode | Gets the exposure mode.
Go2Sensor_ExposureStepAt | Get the exposure step value specified by index
Go2Sensor_ExposureStepCount | Get the number of exposure steps defined
Go2Sensor_ExposureTrainingEnabled | Gets the status of the exposure enabled option.
Go2Sensor_FirmwareVersion | Gets the firmware version installed on this sensor.
Go2Sensor_FrontCameraHeight | Gets the camera region-of-interest height.
Go2Sensor_FrontCameraWidth | Gets the camera region-of-interest width.
Go2Sensor_FrontCameraX | Gets the camera region-of-interest x origin.
Go2Sensor_FrontCameraY | Gets the camera region-of-interest y origin.
Go2Sensor_Id | Gets the device identifier associated with this sensor.
Go2Sensor_IntensityStepIndex | Get the exposure step that will be used for intensity data.
Go2Sensor_IsHost | Reports whether the sensor is currently hosting the connection.
Go2Sensor_IsOnline | Reports whether the sensor is currenly online.
Go2Sensor_Model | Gets the model number associated with this sensor.
Go2Sensor_ModelString | Returns the string representing the sensor model as provided by the firmware.
Go2Sensor_Orientation | Gets the transform orientation identifier.
Go2Sensor_Resolution | Gets the Resolution.
Go2Sensor_ResolutionMax | Gets the maximum valid value for the Resolution setting.
Go2Sensor_ResolutionMin | Gets the minimum valid value for the Resolution setting.
Go2Sensor_Role | Gets the sensor's current role within the system.
Go2Sensor_SetActiveAreaHeight | Sets the active area height.
Go2Sensor_SetActiveAreaLength | Sets the active area Length.
Go2Sensor_SetActiveAreaWidth | Sets the active area width.
Go2Sensor_SetActiveAreaX | Sets the active area x origin.
Go2Sensor_SetActiveAreaY | Sets the active area Y origin.
Go2Sensor_SetActiveAreaZ | Sets the active area z origin.
Go2Sensor_SetExposure | Sets the exposure value.
Go2Sensor_SetExposureDelay | Sets the exposure delay.
Go2Sensor_SetExposureMode | Sets the exposure mode.
Go2Sensor_SetIntensityStepIndex | Set the exposure step that will be used for intensity data. Must be less than ExposureStepCount.
Go2Sensor_SetOrientation | Sets the transform x-offset.
Go2Sensor_SetResolution | Sets the Resolution.
Go2Sensor_SetXAngle | Sets the transform x-angle.
Go2Sensor_SetXOffset | Sets the transform x-offset.
Go2Sensor_SetYAngle | Sets the transform y-angle.
Go2Sensor_SetYOffset | Sets the transform y-offset.
Go2Sensor_SetZAngle | Sets the transform z-angle.
Go2Sensor_SetZOffset | Sets the transform z-offset.
Go2Sensor_SetZResolutionDivider | Sets the current z-resolution divider.
Go2Sensor_XAngle | Gets the transform x-angle.
Go2Sensor_XOffset | Gets the transform x-offset.
Go2Sensor_YAngle | Gets the transform y-angle.
Go2Sensor_YOffset | Gets the transform y-offset.
Go2Sensor_ZAngle | Gets the transform z-angle.
Go2Sensor_ZOffset | Gets the transform z-offset.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference