Gocator API > Go2.Part > Classes > Go2PartStudTipX > Functions

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2PartStudTipX

Go2PartStudTipX Functions

Functions

Function | Description
Go2PartStudTipX_AutoRefRegionEnabled | Reports whether auto reference regions are enabled.
Go2PartStudTipX_AutoTiltCorrectionEnabled | Reports whether auto tilt correction is enabled.
Go2PartStudTipX_BaseHeight | Gets the height of the base of the stud.
Go2PartStudTipX_DecisionMax | Gets the decision threshold maximum value.
Go2PartStudTipX_DecisionMin | Gets the decision threshold minimum value.
Go2PartStudTipX_EnableAutoRefRegion | Enables or disables auto reference regions.
Go2PartStudTipX_EnableAutoTiltCorrection | Enables or disables auto tilt correction.
Go2PartStudTipX_EnableHold | Enables measurement value hold.
Go2PartStudTipX_EnableLink | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement.
Go2PartStudTipX_EnableRefRegions | Enables or disables the optional reference region.
Go2PartStudTipX_EnableRegion | Enables or disables the optional region.
Go2PartStudTipX_EnableSmoothing | Enables measurement value smoothing.
Go2PartStudTipX_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartStudTipX_Id | Gets the unique measurement identifier for the measurement.
Go2PartStudTipX_Link | Gets the measurement id of the linked measurement.
Go2PartStudTipX_LinkEnabled | Reports whether measurement linking is enabled.
Go2PartStudTipX_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2PartStudTipX_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2PartStudTipX_Name | Gets the descriptive name for the measurement.
Go2PartStudTipX_Offset | Gets the measurement value offset.
Go2PartStudTipX_RefRegionAt | Gets the reference region object at the specified index.
Go2PartStudTipX_RefRegionCount | Gets the number of reference regions.
Go2PartStudTipX_RefRegionsEnabled | Returns the current state of the optional reference region.
Go2PartStudTipX_Region | Gets the region object which defines the measurement's ROI.
Go2PartStudTipX_RegionEnabled | Returns the current state of the optional region.
Go2PartStudTipX_Scale | Gets the measurement value scale factor.
Go2PartStudTipX_SetBaseHeight | Sets the height of the base of the stud.
Go2PartStudTipX_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartStudTipX_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartStudTipX_SetId | Sets the unique measurement identifier for the measurement.
Go2PartStudTipX_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartStud_? measurements)
Go2PartStudTipX_SetName | Sets the descriptive name for the measurement.
Go2PartStudTipX_SetOffset | Sets the measurement value offset.
Go2PartStudTipX_SetRefRegionCount | Sets the number of reference regions to use.
Go2PartStudTipX_SetScale | Sets the measurement value scale factor.
Go2PartStudTipX_SetSmoothingWindow | Sets the smoothing window value.
Go2PartStudTipX_SetStudHeight | Sets the height of the stud to measure.
Go2PartStudTipX_SetStudRadius | Sets the radius of the stud to measure.
Go2PartStudTipX_SetTiltXAngle | Sets the X axis tilt angle.
Go2PartStudTipX_SetTiltYAngle | Sets the Y axis tilt angle.
Go2PartStudTipX_SetTipHeight | Sets the height of the tip of the stud.
Go2PartStudTipX_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartStudTipX_SmoothingWindow | Gets the smoothing window value.
Go2PartStudTipX_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartStudTipX_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2PartStudTipX_StudHeight | Gets the height of the stud to measure.
Go2PartStudTipX_StudRadius | Gets the radius of the stud to measure.
Go2PartStudTipX_TiltXAngle | Gets the X axis tilt angle.
Go2PartStudTipX_TiltYAngle | Gets the Y axis tilt angle.
Go2PartStudTipX_TipHeight | Gets the height of the tip of the stud.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference