Gocator API > Go2.Output > Classes > Go2Ethernet > Functions > Go2Ethernet_SetAsciiOperation

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2Ethernet_SetAsciiOperation
Functions
Description

Sets the ASCII operation. When set to GO2_ASCII_ASYNCHRONOUS, the data port will send data asynchronously according to AsciiCustomFormatEnabled. When set to GO2_ASCII_POLLING, no data will be sent unless requested.

C

    Go2Status Go2Ethernet_SetAsciiOperation(Go2Ethernet ethernet, Go2AsciiOperation operation);

Parameters

Parameters | Description
Go2Ethernet ethernet | Go2Ethernet object.
Go2AsciiOperation operation | The ASCII operation.

Returns

Operation status.

File

Go2OutputChannels.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference