Gocator API > Go2.Output > Classes > Go2Analog > Go2Analog Functions

Gocator 1x00 API | Contents | Reference |

Go2Analog Functions Functions
Go2Analog Functions Legend
Functions

Function | Description
Go2Analog_CurrentInvalid | Gets the current output level associated with an invalid measurement.
Go2Analog_CurrentInvalidEnabled | Gets the status of the invalid current enabled option
Go2Analog_CurrentLimitMax | Gets the maximum valid value for CurrentMin, CurrentMax and CurrentInvalid settings.
Go2Analog_CurrentLimitMin | Gets the minimum valid value for CurrentMin, CurrentMax and CurrentInvalid settings.
Go2Analog_CurrentMax | Gets the maximum current output level.
Go2Analog_CurrentMin | Gets the minimum current output level.
Go2Analog_DataScaleMax | Gets the measurement value associated with the maximum output current value.
Go2Analog_DataScaleMin | Gets the measurement value associated with the minimum output current value.
Go2Analog_Delay | Gets the output delay.
Go2Analog_EnableCurrentInvalid | Enables or disables the current output level associated with an invalid measurement. When this is disabled, the output value will be held constant on an invalid measurement
Go2Analog_EnableSchedule | Enables or disables the scheduler for this output
Go2Analog_Event | Gets the event which triggers this output to fire
Go2Analog_OptionAt | Gets the source option at the specified index.
Go2Analog_OptionCount | Gets the number of source options for the specified output type.
Go2Analog_ScheduleEnabled | Gets the enabled state of the scheduler for this output
Go2Analog_SetCurrentInvalid | Sets the current output level associated with an invalid measurement.
Go2Analog_SetCurrentMax | Sets the maximum current output level.
Go2Analog_SetCurrentMin | Sets the minimum current output level.
Go2Analog_SetDataScaleMax | Sets the measurement value associated with the maximum output current value.
Go2Analog_SetDataScaleMin | Sets the measurement value associated with the minimum output current value.
Go2Analog_SetDelay | Sets the delay from exposure until output is triggered, in units based on SyncDomain mm when SyncDomain is distance, us when SyncDomain is time Ignored when SyncDomain is Immediate or when output is Software triggered
Go2Analog_SetEvent | Sets the event which triggers this output to fire
Go2Analog_SetSource | Selects a source type and source identifier for output.
Go2Analog_Source | Gets the selected source identifier.
Go2Analog_SourceType | Gets the selected source type.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference