Gocator API > Go2.Profile > Classes > Go2ProfileGap > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2ProfileGap_Axis | Gets the configured axis along which to measure the gap.
Go2ProfileGap_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileGap_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileGap_EnableHold | Enables measurement value hold.
Go2ProfileGap_EnableLink | Enables or disables measurement linking.
Go2ProfileGap_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileGap_GapWidthMax | Gets the maximum allowable gap size
Go2ProfileGap_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileGap_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileGap_LeftEdge | Gets the edge for the left side
Go2ProfileGap_Link | Gets the measurement id of the linked measurement.
Go2ProfileGap_LinkEnabled | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement. E.g. A Go2PartOpeningX and Go2PartOpeningY measurement can link, but two Go2PartOpeningX measurements can not be linked.
Go2ProfileGap_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2ProfileGap_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2ProfileGap_Name | Gets the descriptive name for the measurement.
Go2ProfileGap_Offset | Gets the measurement value offset.
Go2ProfileGap_ReferenceSide | Gets which of the two edges the measurement is based off of.
Go2ProfileGap_RightEdge | Gets the edge for the right side
Go2ProfileGap_Scale | Gets the measurement value scale factor.
Go2ProfileGap_SetAxis | Determines along which axis to measure the gap.
Go2ProfileGap_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileGap_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileGap_SetGapWidthMax | Sets the maximum allowable gap size.
Go2ProfileGap_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileGap_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2ProfileGap_SetName | Sets the descriptive name for the measurement.
Go2ProfileGap_SetOffset | Sets the measurement value offset.
Go2ProfileGap_SetReferenceSide | Determines which of the two edges to base the measurement off of.
Go2ProfileGap_SetScale | Sets the measurement value scale factor.
Go2ProfileGap_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileGap_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileGap_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileGap_SmoothingWindow | Gets the smoothing window value.
Go2ProfileGap_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileGap_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileGap_Source | Gets the source for profile data used in this measurement.
Go2ProfileGap_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileGap_SourceOptionCount | Gets the number of profile source options for the measurement.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference