Gocator API > Go2.Part > Classes > Go2PartBoundingBoxY > Functions > Go2PartBoundingBoxY_EnableRotation

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2PartBoundingBoxY_EnableRotation
Functions
Description

Enables bounding box rotation. When enabled, the bounding box will rotate according to the major axis of the detected part and measurements will be adjusted accordingly.

C

    Go2Status Go2PartBoundingBoxY_EnableRotation(Go2PartBoundingBoxY measurement, Go2Bool enable);

Parameters

Parameters | Description
Go2PartBoundingBoxY measurement | Go2PartBoundingBoxY object.
Go2Bool enable | GO2_TRUE to enable, or GO2_FALSE to disable.

Returns

Operation status.

File

Go2PartBoundingBoxY.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference