Gocator API > Go2.Data > Values > Go2MeasurementType

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2MeasurementType
Values
Description

Represents an identifier that can be used to distinguish measurement types within a Go2MeasurementData message.

Please note that profile and part measurements are not supported on 1x00 family of sensors. Also, Range measurements are not supported on the 2x00 family of sensors.

C

    enum Go2MeasurementType {
      GO2_MEASUREMENT_TYPE_RANGE_POSITION_Z = 0x80,
      GO2_MEASUREMENT_TYPE_RANGE_DIFFERENCE = 0x81,
      GO2_MEASUREMENT_TYPE_PROFILE_WIDTH = 0x00,
      GO2_MEASUREMENT_TYPE_PROFILE_HEIGHT = 0x01,
      GO2_MEASUREMENT_TYPE_PROFILE_DISTANCE = 0x02,
      GO2_MEASUREMENT_TYPE_PROFILE_CENTER_X = 0x03,
      GO2_MEASUREMENT_TYPE_PROFILE_CENTER_Z = 0x04,
      GO2_MEASUREMENT_TYPE_PROFILE_POSITION_X = 0x05,
      GO2_MEASUREMENT_TYPE_PROFILE_POSITION_Z = 0x06,
      GO2_MEASUREMENT_TYPE_PROFILE_ANGLE_X = 0x13,
      GO2_MEASUREMENT_TYPE_PROFILE_ISECT_X = 0x10,
      GO2_MEASUREMENT_TYPE_PROFILE_ISECT_Z = 0x11,
      GO2_MEASUREMENT_TYPE_PROFILE_ISECT_ANGLE = 0x12,
      GO2_MEASUREMENT_TYPE_PROFILE_ISECT_AREA = 0x20,
      GO2_MEASUREMENT_TYPE_PROFILE_BOX_AREA = 0x21,
      GO2_MEASUREMENT_TYPE_PROFILE_DIFF_AREA = 0x23,
      GO2_MEASUREMENT_TYPE_PROFILE_DIFF_PEAK = 0x24,
      GO2_MEASUREMENT_TYPE_PROFILE_GAP = 0x25,
      GO2_MEASUREMENT_TYPE_PROFILE_FLUSH = 0x26,
      GO2_MEASUREMENT_TYPE_PROFILE_CIRCLE_RADIUS = 0x27,
      GO2_MEASUREMENT_TYPE_PROFILE_CIRCLE_X = 0x28,
      GO2_MEASUREMENT_TYPE_PROFILE_CIRCLE_Z = 0x29,
      GO2_MEASUREMENT_TYPE_PROFILE_LINE_STD_DEV = 0x2A,
      GO2_MEASUREMENT_TYPE_PROFILE_LINE_ERROR_MIN = 0x2B,
      GO2_MEASUREMENT_TYPE_PROFILE_LINE_ERROR_MAX = 0x2C,
      GO2_MEASUREMENT_TYPE_PROFILE_LINE_PERCENTILE = 0x2D,
      GO2_MEASUREMENT_TYPE_PROFILE_GROOVE_X = 0x2E,
      GO2_MEASUREMENT_TYPE_PROFILE_GROOVE_Z = 0x2F,
      GO2_MEASUREMENT_TYPE_PROFILE_GROOVE_WIDTH = 0x31,
      GO2_MEASUREMENT_TYPE_PROFILE_GROOVE_DEPTH = 0x37,
      GO2_MEASUREMENT_TYPE_PROFILE_BRIDGE_VALUE = 0x32,
      GO2_MEASUREMENT_TYPE_PROFILE_STRIP_WIDTH = 0x33,
      GO2_MEASUREMENT_TYPE_PROFILE_STRIP_HEIGHT = 0x34,
      GO2_MEASUREMENT_TYPE_PROFILE_STRIP_X = 0x35,
      GO2_MEASUREMENT_TYPE_PROFILE_STRIP_Z = 0x36,
      GO2_MEASUREMENT_TYPE_SCRIPT = 0x30,
      GO2_MEASUREMENT_TYPE_PART_AREA = 0x40,
      GO2_MEASUREMENT_TYPE_PART_VOLUME = 0x41,
      GO2_MEASUREMENT_TYPE_PART_HEIGHT = 0x42,
      GO2_MEASUREMENT_TYPE_PART_ELLIPSE_MAJOR = 0x46,
      GO2_MEASUREMENT_TYPE_PART_ELLIPSE_MINOR = 0x47,
      GO2_MEASUREMENT_TYPE_PART_ELLIPSE_ANGLE = 0x48,
      GO2_MEASUREMENT_TYPE_PART_ELLIPSE_RATIO = 0x49,
      GO2_MEASUREMENT_TYPE_PART_BOUNDING_BOX_X = 0x4A,
      GO2_MEASUREMENT_TYPE_PART_BOUNDING_BOX_Y = 0x4B,
      GO2_MEASUREMENT_TYPE_PART_BOUNDING_BOX_WIDTH = 0x4C,
      GO2_MEASUREMENT_TYPE_PART_BOUNDING_BOX_LENGTH = 0x4D,
      GO2_MEASUREMENT_TYPE_PART_HOLE_X = 0x4E,
      GO2_MEASUREMENT_TYPE_PART_HOLE_Y = 0x4F,
      GO2_MEASUREMENT_TYPE_PART_HOLE_Z = 0x50,
      GO2_MEASUREMENT_TYPE_PART_HOLE_RADIUS = 0x51,
      GO2_MEASUREMENT_TYPE_PART_STUD_TIP_X = 0x52,
      GO2_MEASUREMENT_TYPE_PART_STUD_TIP_Y = 0x53,
      GO2_MEASUREMENT_TYPE_PART_STUD_TIP_Z = 0x54,
      GO2_MEASUREMENT_TYPE_PART_STUD_BASE_X = 0x55,
      GO2_MEASUREMENT_TYPE_PART_STUD_BASE_Y = 0x56,
      GO2_MEASUREMENT_TYPE_PART_STUD_BASE_Z = 0x57,
      GO2_MEASUREMENT_TYPE_PART_STUD_RADIUS = 0x58,
      GO2_MEASUREMENT_TYPE_PART_OPENING_X = 0x59,
      GO2_MEASUREMENT_TYPE_PART_OPENING_Y = 0x5A,
      GO2_MEASUREMENT_TYPE_PART_OPENING_Z = 0x5B,
      GO2_MEASUREMENT_TYPE_PART_OPENING_ANGLE = 0x5C,
      GO2_MEASUREMENT_TYPE_PART_OPENING_LENGTH = 0x5D,
      GO2_MEASUREMENT_TYPE_PART_OPENING_WIDTH = 0x5E,
      GO2_MEASUREMENT_TYPE_PART_POSITION_X = 0x5F,
      GO2_MEASUREMENT_TYPE_PART_POSITION_Y = 0x60,
      GO2_MEASUREMENT_TYPE_PART_POSITION_Z = 0x61,
      GO2_MEASUREMENT_TYPE_PART_PLANE_X_ANGLE = 0x62,
      GO2_MEASUREMENT_TYPE_PART_PLANE_Y_ANGLE = 0x63,
      GO2_MEASUREMENT_TYPE_PART_PLANE_Z_OFFSET = 0x64,
      GO2_MEASUREMENT_TYPE_PART_TEXTURE_ROUGHNESS = 0x65,
      GO2_MEASUREMENT_TYPE_PART_TEXTURE_INVALID_COUNT = 0x66
    };

Members

Members | Description
GO2_MEASUREMENT_TYPE_RANGE_POSITION_Z = 0x80 | Range position Z measurement data id.
GO2_MEASUREMENT_TYPE_RANGE_DIFFERENCE = 0x81 | Range difference measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_WIDTH = 0x00 | Profile width measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_HEIGHT = 0x01 | Profile height measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_DISTANCE = 0x02 | Profile distance measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_CENTER_X = 0x03 | Profile center X measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_CENTER_Z = 0x04 | Profile center Z measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_POSITION_X = 0x05 | Profile position X measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_POSITION_Z = 0x06 | Profile position Z measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_ANGLE_X = 0x13 | Profile angle X measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_ISECT_X = 0x10 | Profile intersect X measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_ISECT_Z = 0x11 | Profile intersect Z measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_ISECT_ANGLE = 0x12 | Profile intersect angle measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_ISECT_AREA = 0x20 | Profile intesect area measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_BOX_AREA = 0x21 | Profile box area measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_DIFF_AREA = 0x23 | Profile difference area measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_DIFF_PEAK = 0x24 | Profile difference peak measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_GAP = 0x25 | Profile gap measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_FLUSH = 0x26 | Profile flush measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_CIRCLE_RADIUS = 0x27 | Profile circle radius measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_CIRCLE_X = 0x28 | Profile circle X measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_CIRCLE_Z = 0x29 | Profile circle Z measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_LINE_STD_DEV = 0x2A | Profile line std dev measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_LINE_ERROR_MIN = 0x2B | Profile line error min measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_LINE_ERROR_MAX = 0x2C | Profile line error max measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_LINE_PERCENTILE = 0x2D | Profile line percentile measurement data id.
GO2_MEASUREMENT_TYPE_PROFILE_GROOVE_X = 0x2E | Profile groove X data id.
GO2_MEASUREMENT_TYPE_PROFILE_GROOVE_Z = 0x2F | Profile groove Z data id.
GO2_MEASUREMENT_TYPE_PROFILE_GROOVE_WIDTH = 0x31 | Profile groove width data id.
GO2_MEASUREMENT_TYPE_PROFILE_GROOVE_DEPTH = 0x37 | Profile groove width data id.
GO2_MEASUREMENT_TYPE_PROFILE_BRIDGE_VALUE = 0x32 | Profile bridge value data id.
GO2_MEASUREMENT_TYPE_PROFILE_STRIP_WIDTH = 0x33 | Profile strip width data id.
GO2_MEASUREMENT_TYPE_PROFILE_STRIP_HEIGHT = 0x34 | Profile strip height data id.
GO2_MEASUREMENT_TYPE_PROFILE_STRIP_X = 0x35 | Profile strip X data id.
GO2_MEASUREMENT_TYPE_PROFILE_STRIP_Z = 0x36 | Profile strip Z data id.
GO2_MEASUREMENT_TYPE_SCRIPT = 0x30 | Script measurement output.
GO2_MEASUREMENT_TYPE_PART_AREA = 0x40 | Part area measurement data id.
GO2_MEASUREMENT_TYPE_PART_VOLUME = 0x41 | Part volume measurement data id.
GO2_MEASUREMENT_TYPE_PART_HEIGHT = 0x42 | Part height measurement data id.
GO2_MEASUREMENT_TYPE_PART_ELLIPSE_MAJOR = 0x46 | Part ellipse major measurement data id.
GO2_MEASUREMENT_TYPE_PART_ELLIPSE_MINOR = 0x47 | Part ellipse minor measurement data id.
GO2_MEASUREMENT_TYPE_PART_ELLIPSE_ANGLE = 0x48 | Part ellipse angle measurement data id.
GO2_MEASUREMENT_TYPE_PART_ELLIPSE_RATIO = 0x49 | Part ellipse ratio measurement data id.
GO2_MEASUREMENT_TYPE_PART_BOUNDING_BOX_X = 0x4A | Part bounding box X measurement data id.
GO2_MEASUREMENT_TYPE_PART_BOUNDING_BOX_Y = 0x4B | Part bounding box Y measurement data id.
GO2_MEASUREMENT_TYPE_PART_BOUNDING_BOX_WIDTH = 0x4C | Part bounding box width measurement data id.
GO2_MEASUREMENT_TYPE_PART_BOUNDING_BOX_LENGTH = 0x4D | Part bounding box length measurement data id.
GO2_MEASUREMENT_TYPE_PART_HOLE_X = 0x4E | Part hole x measurement data id.
GO2_MEASUREMENT_TYPE_PART_HOLE_Y = 0x4F | Part hole y measurement data id.
GO2_MEASUREMENT_TYPE_PART_HOLE_Z = 0x50 | Part hole z measurement data id.
GO2_MEASUREMENT_TYPE_PART_HOLE_RADIUS = 0x51 | Part hole radius measurement data id.
GO2_MEASUREMENT_TYPE_PART_STUD_TIP_X = 0x52 | Part stud tip x measurement data id.
GO2_MEASUREMENT_TYPE_PART_STUD_TIP_Y = 0x53 | Part stud tip y measurement data id.
GO2_MEASUREMENT_TYPE_PART_STUD_TIP_Z = 0x54 | Part stud tip z measurement data id.
GO2_MEASUREMENT_TYPE_PART_STUD_BASE_X = 0x55 | Part stud base x measurement data id.
GO2_MEASUREMENT_TYPE_PART_STUD_BASE_Y = 0x56 | Part stud base y measurement data id.
GO2_MEASUREMENT_TYPE_PART_STUD_BASE_Z = 0x57 | Part stud base z measurement data id.
GO2_MEASUREMENT_TYPE_PART_STUD_RADIUS = 0x58 | Part stud radius measurement data id.
GO2_MEASUREMENT_TYPE_PART_OPENING_X = 0x59 | Part opening x measurement data id.
GO2_MEASUREMENT_TYPE_PART_OPENING_Y = 0x5A | Part opening y measurement data id.
GO2_MEASUREMENT_TYPE_PART_OPENING_Z = 0x5B | Part opening z measurement data id.
GO2_MEASUREMENT_TYPE_PART_OPENING_ANGLE = 0x5C | Part opening angle measurement data id.
GO2_MEASUREMENT_TYPE_PART_OPENING_LENGTH = 0x5D | Part opening width measurement data id.
GO2_MEASUREMENT_TYPE_PART_OPENING_WIDTH = 0x5E | Part opening length measurement data id.
GO2_MEASUREMENT_TYPE_PART_POSITION_X = 0x5F | Part opening position X measurement data id.
GO2_MEASUREMENT_TYPE_PART_POSITION_Y = 0x60 | Part opening position Y measurement data id.
GO2_MEASUREMENT_TYPE_PART_POSITION_Z = 0x61 | Part opening position Z measurement data id.
GO2_MEASUREMENT_TYPE_PART_PLANE_X_ANGLE = 0x62 | Part plane X angle measurement data id.
GO2_MEASUREMENT_TYPE_PART_PLANE_Y_ANGLE = 0x63 | Part plane Y angle measurement data id.
GO2_MEASUREMENT_TYPE_PART_PLANE_Z_OFFSET = 0x64 | Part plane Z offset measurement data id.
GO2_MEASUREMENT_TYPE_PART_TEXTURE_ROUGHNESS = 0x65 | Part texture roughness measurement data id.
GO2_MEASUREMENT_TYPE_PART_TEXTURE_INVALID_COUNT = 0x66 | Part texture invalid count measurement data id.

File

Go2Measurement.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference