Gocator API > Go2 > Classes > Go2Sensor > Functions > Go2Sensor_ActiveAreaXMin

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2Sensor_ActiveAreaXMin
Functions
Description

Gets the minimum valid value for the ActiveAreaX setting.

C

    Go2Double Go2Sensor_ActiveAreaXMin(Go2Sensor sensor);

Parameters

Parameters | Description
Go2Sensor sensor | Go2Sensor object.

Returns

Minimum valid ActiveAreaX value (mm).

File

Go2Sensor.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference