Gocator API > Go2.Part > Classes > Go2PartOpeningY > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2PartOpeningY_AngleTolerance | Gets the tolerance between the nominal Angle and the detected hole size.
Go2PartOpeningY_AutoRefRegionEnabled | Reports whether auto reference regions are enabled.
Go2PartOpeningY_AutoTiltCorrectionEnabled | Reports whether auto tilt correction is enabled.
Go2PartOpeningY_DecisionMax | Gets the decision threshold maximum value.
Go2PartOpeningY_DecisionMin | Gets the decision threshold minimum value.
Go2PartOpeningY_EnableAutoRefRegion | Enables or disables auto reference regions.
Go2PartOpeningY_EnableAutoTiltCorrection | Enables or disables auto tilt correction.
Go2PartOpeningY_EnableHold | Enables measurement value hold.
Go2PartOpeningY_EnableLink | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement.
Go2PartOpeningY_EnablePartialDetection | Enables or disables partial hole detection.
Go2PartOpeningY_EnableRefRegions | Enables or disables the optional reference region.
Go2PartOpeningY_EnableRegion | Enables or disables the optional region.
Go2PartOpeningY_EnableSmoothing | Enables measurement value smoothing.
Go2PartOpeningY_HoldEnabled | Reports whether value hold is currently enabled.
Go2PartOpeningY_Id | Gets the unique measurement identifier for the measurement.
Go2PartOpeningY_LengthTolerance | Gets the tolerance between the nominal Length and the detected hole size.
Go2PartOpeningY_Link | Gets the measurement id of the linked measurement.
Go2PartOpeningY_LinkEnabled | Reports whether measurement linking is enabled.
Go2PartOpeningY_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2PartOpeningY_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2PartOpeningY_Name | Gets the descriptive name for the measurement.
Go2PartOpeningY_NominalAngle | Gets the nominal Angle of the hole to measure.
Go2PartOpeningY_NominalLength | Gets the nominal Length of the hole to measure.
Go2PartOpeningY_NominalRadius | Gets the nominal Radius of the hole to measure.
Go2PartOpeningY_NominalWidth | Gets the nominal Width of the hole to measure.
Go2PartOpeningY_Offset | Gets the measurement value offset.
Go2PartOpeningY_PartialDetectionEnabled | Gets the current partial hole detection value.
Go2PartOpeningY_RefRegionAt | Gets the reference region object at the specified index.
Go2PartOpeningY_RefRegionCount | Gets the number of reference regions.
Go2PartOpeningY_RefRegionsEnabled | Returns the current state of the optional reference region.
Go2PartOpeningY_Region | Gets the region object which defines the measurement's ROI.
Go2PartOpeningY_RegionEnabled | Returns the current state of the optional region.
Go2PartOpeningY_Scale | Gets the measurement value scale factor.
Go2PartOpeningY_SetAngleTolerance | Sets the tolerance between the nominal Angle and the detected hole size.
Go2PartOpeningY_SetDecisionMax | Sets the decision threshold maximum value.
Go2PartOpeningY_SetDecisionMin | Sets the decision threshold minimum value.
Go2PartOpeningY_SetId | Sets the unique measurement identifier for the measurement.
Go2PartOpeningY_SetLengthTolerance | Sets the tolerance between the nominal Length and the detected hole size.
Go2PartOpeningY_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2PartOpeningY_SetName | Sets the descriptive name for the measurement.
Go2PartOpeningY_SetNominalAngle | Sets the nominal Angle of the hole to measure.
Go2PartOpeningY_SetNominalLength | Sets the nominal Length of the hole to measure.
Go2PartOpeningY_SetNominalRadius | Sets the nominal Radius of the hole to measure.
Go2PartOpeningY_SetNominalWidth | Sets the nominal Width of the hole to measure.
Go2PartOpeningY_SetOffset | Sets the measurement value offset.
Go2PartOpeningY_SetRefRegionCount | Sets the number of reference regions to use.
Go2PartOpeningY_SetScale | Sets the measurement value scale factor.
Go2PartOpeningY_SetSmoothingWindow | Sets the smoothing window value.
Go2PartOpeningY_SetTiltXAngle | Sets the X axis tilt angle.
Go2PartOpeningY_SetTiltYAngle | Sets the Y axis tilt angle.
Go2PartOpeningY_SetType | Sets the type of opening y measurement to be measured.
Go2PartOpeningY_SetWidthTolerance | Sets the tolerance between the nominal width and the detected hole size.
Go2PartOpeningY_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2PartOpeningY_SmoothingWindow | Gets the smoothing window value.
Go2PartOpeningY_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2PartOpeningY_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2PartOpeningY_TiltXAngle | Gets the X axis tilt angle.
Go2PartOpeningY_TiltYAngle | Gets the Y axis tilt angle.
Go2PartOpeningY_Type | Gets the type of opening y measurement to be measured.
Go2PartOpeningY_WidthTolerance | Gets the tolerance between the nominal width and the detected hole size.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference