Gocator API > Go2 > Values > Go2SensorOrientation

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2SensorOrientation
Values
Description

Represents the sensors orientation

C

    enum Go2SensorOrientation {
      GO2_SENSOR_ORIENTATION_NORMAL = 0,
      GO2_SENSOR_ORIENTATION_REVERSE = 1
    };

Members

Members | Description
GO2_SENSOR_ORIENTATION_NORMAL = 0 | Normal mounting
GO2_SENSOR_ORIENTATION_REVERSE = 1 | Reverse mounting (180 deg rotated about y-axis)

File

Go2Sensor.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference