Gocator API > Go2.Output > Values > Go2DigitalEvent

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2DigitalEvent
Values
Description

Represents the event which triggers this output.

C

    enum Go2DigitalEvent {
      GO2_DIGITAL_CONTROL_EVENT_NONE = 0,
      GO2_DIGITAL_CONTROL_EVENT_MEASUREMENT = 1,
      GO2_DIGITAL_CONTROL_EVENT_SOFTWARE = 2,
      GO2_DIGITAL_CONTROL_EVENT_CALIBRATION = 3,
      GO2_DIGITAL_CONTROL_EVENT_EXPOSURE = 4
    };

Members

Members | Description
GO2_DIGITAL_CONTROL_EVENT_NONE = 0 | Output is disabled.
GO2_DIGITAL_CONTROL_EVENT_MEASUREMENT = 1 | Output is measurement driven.
GO2_DIGITAL_CONTROL_EVENT_SOFTWARE = 2 | Output is software driven.
GO2_DIGITAL_CONTROL_EVENT_CALIBRATION = 3 | Output represents the calibration state. Scheduling is disabled.
GO2_DIGITAL_CONTROL_EVENT_EXPOSURE = 4 | Output triggers on exposure.

File

Go2Api.h

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference