Gocator API > Go2 > Classes > Go2System > Functions > Go2System_GetAddress

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2System_GetAddress
Functions
Description

Locates a Gocator sensor by id (serial number) and reports its network address settings.

C

    Go2Status Go2System_GetAddress(Go2UInt32 deviceId, Go2AddressInfo* address);

Parameters

Parameters | Description
Go2UInt32 deviceId | Serial number of the sensor.
Go2AddressInfo* address | Receives current address configuration if the sensor was found.

Returns

Operation status.

Remarks

This function uses UDP broadcast messages to locate Gocator sensors. The sensors and client may be on different subnets.

File

Go2System.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference