Gocator API > Go2 > Values > Go2ConnectionType

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2ConnectionType
Values
Description

Represents the type of system interconnection.

C

    enum Go2ConnectionType {
      GO2_CONNECTION_TYPE_STANDALONE = 0,
      GO2_CONNECTION_TYPE_MASTER_100 = 1,
      GO2_CONNECTION_TYPE_MASTER_200 = 2,
      GO2_CONNECTION_TYPE_MASTER_400 = 3,
      GO2_CONNECTION_TYPE_MASTER_800 = 4,
      GO2_CONNECTION_TYPE_MASTER_1200 = 5,
      GO2_CONNECTION_TYPE_MASTER_2400 = 6
    };

Members

Members | Description
GO2_CONNECTION_TYPE_STANDALONE = 0 | No Master (open wire).
GO2_CONNECTION_TYPE_MASTER_100 = 1 | Master 100.
GO2_CONNECTION_TYPE_MASTER_200 = 2 | Master 200.
GO2_CONNECTION_TYPE_MASTER_400 = 3 | Master 400.
GO2_CONNECTION_TYPE_MASTER_800 = 4 | Master 800.
GO2_CONNECTION_TYPE_MASTER_1200 = 5 | Master 1200.
GO2_CONNECTION_TYPE_MASTER_2400 = 6 | Master 2400.

File

Go2Api.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference