Gocator API > Go2 > Values > Go2EncoderPeriodMinSource

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2EncoderPeriodMinSource
Values
Description

Determines what is currently limiting the minimum encoder period.

C

    enum Go2EncoderPeriodMinSource {
      GO2_ENCODER_PERIOD_MIN_SOURCE_RESOLUTION = 0,
      GO2_ENCODER_PERIOD_MIN_SOURCE_PART_DETECTION = 1
    };

Members

Members | Description
GO2_ENCODER_PERIOD_MIN_SOURCE_RESOLUTION = 0 | Limited by encoder resolution.
GO2_ENCODER_PERIOD_MIN_SOURCE_PART_DETECTION = 1 | Limited by part detection logic.

File

Go2Api.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference