Gocator API > Go2.Data > Classes > Go2RangeData > Functions

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Functions
Functions Go2RangeData

Go2RangeDataFunctions

Functions

Function | Description
Go2RangeData_Exposure | Gets the exposure time of the profile data. Set to 0 if from multiple exposures or sensors are used.
Go2RangeData_Range | Gets the range data in system units. The calculation for each point is: X: 0 Z: ZOffset + range * ZResolution Invalid ranges are equal to GO2_INVALID_RANGE
Go2RangeData_Source | Gets the source for the profile data.
Go2RangeData_ZOffset | Gets the z offset of the profile data. Will always be zero as range data is returned from the sensor with offsets applied. This value does not bear any relationship to the configured active area.
Go2RangeData_ZResolution | Gets the z resolution of the profile data. This is a scaling factor used to convert profile data into actual units (mm). This value does not bear any relationship to the configured system Z resolution.

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference