Gocator API > Go2 > Classes > Go2System > Functions > Go2System_ScheduleDigitalOutput

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2System_ScheduleDigitalOutput
Functions
Description

Schedules a digital output. Requires that the output be configured to trigger on software control

C

    Go2Status Go2System_ScheduleDigitalOutput(Go2System system, Go2Digital digital, Go2Int64 target, Go2Int64 value);

Parameters

Parameters | Description
Go2System system | Go2System object.
Go2Digital digital | Go2Digital object.
Go2Int64 target | The time or position target (uS or ticks), depending on Go2System_SystemDomain. Ignored if Go2Digital_ScheduleEnabled is false or Go2Digital_SignalType is pulsed.
Go2Int64 value | The value of scheduled output (0-Low or 1-High). Ignored if output Go2Digital_SignalType is pulsed.

Returns

Operation status.

File

Go2System.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference