Gocator API > Go2 > Classes > Go2System > Functions > Go2System_ScheduledStart

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2System_ScheduledStart
Functions
Description

Schedules the system to start at the specified time or location. Uses the trigger mode of the system to determine which target to use, defaulting to time for randomly occuring trigger types. This command changes the state of the sensor to running immediately, but the system doesn't actually begin until the target is met.

C

    Go2Status Go2System_ScheduledStart(Go2System system, Go2Int64 timeTarget, Go2Int64 encoderTarget);

Parameters

Parameters | Description
Go2System system | Go2System object.
Go2Int64 timeTarget | Specify start time target (uS).
Go2Int64 encoderTarget | Specify start encoder target (ticks).

Returns

Operation status.

File

Go2System.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference