Gocator API > Go2 > Values > Go2SensorPairState

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2SensorPairState
Values
Description

Represents the pair state of a sensor

C

    enum Go2SensorPairState {
      GO2_SENSOR_PAIR_STATE_INVALID = 0,
      GO2_SENSOR_PAIR_STATE_CONNECTED = 1,
      GO2_SENSOR_PAIR_STATE_MISSING = 2,
      GO2_SENSOR_PAIR_STATE_ERROR = 3
    };

Members

Members | Description
GO2_SENSOR_PAIR_STATE_INVALID = 0 | This sensor is not assigned, or control connection is established to this sensor.
GO2_SENSOR_PAIR_STATE_CONNECTED = 1 | Pair is connected
GO2_SENSOR_PAIR_STATE_MISSING = 2 | Paired sensor is missing
GO2_SENSOR_PAIR_STATE_ERROR = 3 | Error state - can't pair for some reason

File

Go2Api.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference