Gocator API > Go2 > Values > Go2Orientation

Gocator 3x00 API | Contents | Reference | Previous | Up | Next

Go2Orientation
Values
Description

Represents a sensor orientation type.

C

    enum Go2Orientation {
      GO2_ORIENTATION_ISOLATED = 0,
      GO2_ORIENTATION_WIDE = 1,
      GO2_ORIENTATION_STAGGERED = 2,
      GO2_ORIENTATION_OPPOSITE = 3
    };

Members

Members | Description
GO2_ORIENTATION_ISOLATED = 0 | Isolated sensor orientation.
GO2_ORIENTATION_WIDE = 1 | Wide sensor orientation.
GO2_ORIENTATION_STAGGERED = 2 | Staggered sensor orientation. Deprecated, sensor will fail to start
GO2_ORIENTATION_OPPOSITE = 3 | Opposite sensor orientation.

File

Go2Api.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference