Gocator API > Go2 > Values > Go2Mode

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2Mode
Values
Description

Represents an operation mode.

C

    enum Go2Mode {
      GO2_MODE_UNKNOWN,
      GO2_MODE_VIDEO,
      GO2_MODE_RANGE_MEASUREMENT,
      GO2_MODE_PROFILE_TEMPLATE,
      GO2_MODE_PROFILE_MEASUREMENT,
      GO2_MODE_PART_TEMPLATE,
      GO2_MODE_PART_MEASUREMENT,
      GO2_MODE_RAW_PROFILE,
      GO2_MODE_EXPOSURE_CAL,
      GO2_MODE_ALIGN_CAL,
      GO2_MODE_TRAVEL_CAL,
      GO2_MODE_ROLINE,
      GO2_MODE_REFERENCE_IMAGE,
      GO2_MODE_CUSTOM
    };

Members

Members | Description
GO2_MODE_UNKNOWN | Unknown operation mode.
GO2_MODE_VIDEO | Video mode.
GO2_MODE_RANGE_MEASUREMENT | Range measurement mode. Supported only on 1x00 series sensors.
GO2_MODE_PROFILE_TEMPLATE | Profile template registration mode. Supported only on 2x00 series sensors.
GO2_MODE_PROFILE_MEASUREMENT | Profile measurement mode. Supported only on 2x00 series sensors.
GO2_MODE_PART_TEMPLATE | Part template registration mode. Supported only on 2x00 series sensors.
GO2_MODE_PART_MEASUREMENT | Part measurement mode. Supported only on 2x00 and 3x00 series sensors.
GO2_MODE_RAW_PROFILE | Raw Profile mode. Supported only on 2x00 series sensors.
GO2_MODE_EXPOSURE_CAL | Exposure calibration mode.
GO2_MODE_ALIGN_CAL | Alignment calibration mode.
GO2_MODE_TRAVEL_CAL | Travel calibration mode.
GO2_MODE_ROLINE | Roline mode. Supported only on specialized sensors.
GO2_MODE_REFERENCE_IMAGE | Reference Image mode.
GO2_MODE_CUSTOM | Custom mode. Supported only on sensors utilizing the Gocator Base Library.

File

Go2Api.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference