Gocator API > Go2 > Classes > Go2Sensor > Functions > Go2Sensor_ActiveAreaHeight

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2Sensor_ActiveAreaHeight
Functions
Description

Gets the active area height.

C

    Go2Double Go2Sensor_ActiveAreaHeight(Go2Sensor sensor);

Parameters

Parameters | Description
Go2Sensor sensor | Go2Sensor object.

Returns

Active area height (mm).

File

Go2Sensor.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference