Gocator API > Go2.Output > Classes > Go2Analog > Go2Analog Functions > Go2Analog_SetDelay

Gocator 1x00 API | Contents | Reference | Previous | Up | Next

Go2Analog_SetDelay
Go2Analog Functions
Description

Sets the delay from exposure until output is triggered, in units based on SyncDomain mm when SyncDomain is distance, us when SyncDomain is time Ignored when SyncDomain is Immediate or when output is Software triggered

C

    Go2Status Go2Analog_SetDelay(Go2Analog analog, Go2Int64 delay);

Parameters

Parameters | Description
Go2Analog analog | Go2Analog object.
Go2Int64 delay | The delay (us or mm)

Returns

Operation status.

File

Go2OutputChannels.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference