Gocator API > Go2.Profile > Values > Go2GapAxis

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2GapAxis
Values
Description

Repesents a profile gap measurement axis

C

    enum Go2GapAxis {
      GO2_GAP_AXIS_EDGE = 0,
      GO2_GAP_AXIS_SURFACE = 1,
      GO2_GAP_AXIS_DISTANCE = 2
    };

Members

Members | Description
GO2_GAP_AXIS_EDGE = 0 | Measure the gap along the edge normal
GO2_GAP_AXIS_SURFACE = 1 | Measure the gap along the surface line
GO2_GAP_AXIS_DISTANCE = 2 | Measure the shortest distance between the two edges

File

Go2ProfileTypes.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference