Gocator API > Go2 > Values > Go2SensorRole

Gocator 2x00 API | Contents | Reference | Previous | Up | Next

Go2SensorRole
Values
Description

Represents the current role of a sensor within a sensor system.

C

    enum Go2SensorRole {
      GO2_SENSOR_ROLE_INVALID = 0,
      GO2_SENSOR_ROLE_MAIN = 1,
      GO2_SENSOR_ROLE_BUDDY = 2,
      GO2_SENSOR_ROLE_UNASSIGNED = 3,
      GO2_SENSOR_ROLE_UNAVAILABLE = 4
    };

Members

Members | Description
GO2_SENSOR_ROLE_INVALID = 0 | Invalid role; occurs when control connection is established to buddy.
GO2_SENSOR_ROLE_MAIN = 1 | Main sensor.
GO2_SENSOR_ROLE_BUDDY = 2 | Buddy sensor.
GO2_SENSOR_ROLE_UNASSIGNED = 3 | Potential buddy sensor, not yet assigned.
GO2_SENSOR_ROLE_UNAVAILABLE = 4 | Not a potential buddy, already assigned to another pair

File

Go2Api.h

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference