Gocator API > Go2.Profile > Classes > Go2ProfileStripHeight > Functions

Gocator 2x00 API | Contents | Reference |

Functions
Functions Legend
Functions

Function | Description
Go2ProfileStripHeight_Area | Gets the region of interest.
Go2ProfileStripHeight_BaseType | Gets the base type of the strip to search for.
Go2ProfileStripHeight_DecisionMax | Gets the decision threshold maximum value.
Go2ProfileStripHeight_DecisionMin | Gets the decision threshold minimum value.
Go2ProfileStripHeight_EdgeHeightMin | Gets the minimum height for an edge to be considered.
Go2ProfileStripHeight_EdgeSupportWidth | Gets the width of the search window to use when detecting edges.
Go2ProfileStripHeight_EdgeTransitionWidth | Gets the width of the expected edge transition.
Go2ProfileStripHeight_EdgeTransitionWidthMax | Gets the maximum value allowable for the edge transition.
Go2ProfileStripHeight_EnableHold | Enables measurement value hold.
Go2ProfileStripHeight_EnableLeftEdgeType | Enables or disables detection of the specified left edge type.
Go2ProfileStripHeight_EnableLink | Enables or disables measurement linking.
Go2ProfileStripHeight_EnableRightEdgeType | Enables or disables detection of the specified right edge type.
Go2ProfileStripHeight_EnableSmoothing | Enables measurement value smoothing.
Go2ProfileStripHeight_EnableTilt | Enables or disables tilt correction.
Go2ProfileStripHeight_HoldEnabled | Reports whether value hold is currently enabled.
Go2ProfileStripHeight_Id | Gets the unique measurement identifier for the measurement.
Go2ProfileStripHeight_LeftEdgeTypeEnabled | Determines whether the specified left edge type is enabled for detection.
Go2ProfileStripHeight_Link | Gets the measurement id of the linked measurement.
Go2ProfileStripHeight_LinkEnabled | Enables measurement linking. When enabled, another measurement of the same base type can be linked, provided that it is a different measurement. E.g. A Go2PartOpeningX and Go2PartOpeningY measurement can link, but two Go2PartOpeningX measurements can not be linked.
Go2ProfileStripHeight_LinkOptionAt | Gets the link-able measurement id at the specified index.
Go2ProfileStripHeight_LinkOptionCount | Gets the number of link-able measurement IDs.
Go2ProfileStripHeight_Location | Gets what location on the strip to return the position of.
Go2ProfileStripHeight_Name | Gets the descriptive name for the measurement.
Go2ProfileStripHeight_Offset | Gets the measurement value offset.
Go2ProfileStripHeight_RightEdgeTypeEnabled | Determines whether the specified right edge type is enabled for detection.
Go2ProfileStripHeight_Scale | Gets the measurement value scale factor.
Go2ProfileStripHeight_SelectN | Gets the N-th strip to select when selectType is GO2_PROFILE_STRIP_SELECT_LEFT or GO2_PROFILE_STRIP_SELECT_RIGHT.
Go2ProfileStripHeight_SelectType | Gets the select type.
Go2ProfileStripHeight_SetBaseType | Sets the base type of the strip to search for.
Go2ProfileStripHeight_SetDecisionMax | Sets the decision threshold maximum value.
Go2ProfileStripHeight_SetDecisionMin | Sets the decision threshold minimum value.
Go2ProfileStripHeight_SetEdgeHeightMin | Sets the minimum height for an edge to be considered.
Go2ProfileStripHeight_SetEdgeSupportWidth | Sets the width of the search window to use when detecting edges.
Go2ProfileStripHeight_SetEdgeTransitionWidth | Sets the width of the expected edge transition.
Go2ProfileStripHeight_SetId | Sets the unique measurement identifier for the measurement.
Go2ProfileStripHeight_SetLink | Sets the measurement id to which this measurement should link. Linked measurements must: -link to a valid measurement id -not link to themselves -not link to a measurement that is already linked -link only to measurements of the same basic type (eg, all PartOpening_? measurements)
Go2ProfileStripHeight_SetLocation | Sets what location on the strip to return the position of.
Go2ProfileStripHeight_SetName | Sets the descriptive name for the measurement.
Go2ProfileStripHeight_SetOffset | Sets the measurement value offset.
Go2ProfileStripHeight_SetScale | Sets the measurement value scale factor.
Go2ProfileStripHeight_SetSelectN | Sets the N-th strip to select when selectType is GO2_PROFILE_STRIP_SELECT_LEFT or GO2_PROFILE_STRIP_SELECT_RIGHT.
Go2ProfileStripHeight_SetSelectType | Sets the select type.
Go2ProfileStripHeight_SetSmoothingWindow | Sets the smoothing window value.
Go2ProfileStripHeight_SetSource | Sets the source for profile data used in this measurement.
Go2ProfileStripHeight_SetVoidMax | Sets the maximum width of the void that will be ignored.
Go2ProfileStripHeight_SetWidthMin | Sets the minimum width for a strip to be considered.
Go2ProfileStripHeight_SmoothingEnabled | Reports whether value smoothing is currently enabled.
Go2ProfileStripHeight_SmoothingWindow | Gets the smoothing window value.
Go2ProfileStripHeight_SmoothingWindowMax | Gets the maximum smoothing window value.
Go2ProfileStripHeight_SmoothingWindowMin | Gets the minimum smoothing window value.
Go2ProfileStripHeight_Source | Gets the source for profile data used in this measurement.
Go2ProfileStripHeight_SourceOptionAt | Gets the profile source option at the specified index.
Go2ProfileStripHeight_SourceOptionCount | Gets the number of profile source options for the measurement.
Go2ProfileStripHeight_TiltEnabled | Determines whether tilt correction is enabled.
Go2ProfileStripHeight_VoidMax | Gets the maximum width of the void that will be ignored.
Go2ProfileStripHeight_VoidMaxLimitMax | Gets the limit for the VoidMax property.
Go2ProfileStripHeight_WidthMin | Gets the minimum width for a strip to be considered.

Created with a commercial version of Doc-O-Matic. In order to make this message disappear you need to register this software. If you have problems registering this software please contact us at support@toolsfactory.com.

Copyright (c) 2013 by LMI Technologies Inc. All rights reserved.
Contents | Reference